{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":5,"rows_kept":5,"merged":[[0,0,0,4],[7,0,8,0],[7,1,8,1]],"flags":["formulas_cached_only"]}
["科创成果汇总表"]
["序号","单位名称","项目名称","内容概述","备  注"]
["例：","上海***公司","新型纳米铝电解电容器","    该项目产品通过改善电容器核心材料“工作电解液”，采用纳米材料添加剂使电解液性能显著提升，并以新型的卷绕工艺，提高电容器寿命及损耗角正切值；该电解液的应用不仅大大提升了电容器使用寿命，同时较传统的电容器明显降低了电容器的损耗，漏电流、耐打纹波特性大大增强，其各方面性能远远高于传统工作电解液；其良好的浸润性、耐纹波性、高温稳定性、修复性能加上特殊的卷绕工艺，使高比容箔能稳定工作，增大单位体积的容量。产品经与日本NCC 黑金刚电容器对比后，各项指标均已超越。","获第八届上海市发明创造专利奖实用新型专利奖；\n达到国际先进水平，处于行业领先地位。"]
[1]
[2]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}